**Jobsheet 1**

**Using Wireshark to Observe the TCP 3-Way**

**Handshak**



Mata Kuliah : Keamanan cyber

Disusun oleh:

Nama : Muhammad Aprilianto Putra

No : 13


**PROGRAM STUDI TEKNIK INFORMATIKA JURUSAN TEKNIK ELEKTRO**

**POLITEKNIK NEGERI SEMARANG 2022**



Lab - Using Wireshark to Observe the TCP 3-Way Handshake

# Mininet Topology



**Objectives**

**Part 1: Prepare the Hosts to Capture the Traffic Part 2: Analyze the Packets using Wireshark Part 3: View the Packets using tcpdump**

# Background / Scenario

In this lab, you will use Wireshark to capture and examine packets generated between the PC browser using the HyperText Transfer Protocol (HTTP) and a web server, such as [www.google.com.](http://www.google.com/) When an application, such as HTTP or File Transfer Protocol (FTP) first starts on a host, TCP uses the three-way handshake to establish a reliable TCP session between the two hosts. For example, when a PC uses a web browser to surf the internet, a three-way handshake is initiated, and a session is established between the PC host and web server. A PC can have multiple, simultaneous, active TCP sessions with various web sites.

# Required Resources


* CyberOps Workstation virtual machine

# Instructions

**Part 1: Prepare the Hosts to Capture the Traffic**

1. Start the CyberOps VM. Log in with username **analyst** and the password **cyberops**.
2. Start Mininet.

[analyst@secOps ~]$ **sudo lab.support.files/scripts/cyberops\_topo.py**


****

1. Start host H1 and H4 in Mininet.

\*\*\* Starting CLI:

mininet> **xterm H1**

mininet> **xterm H4**


****

1. Start the web server on H4.

[root@secOps analyst]#

### /home/analyst/lab.support.files/scripts/reg\_server\_start.sh

### 




1. For security purposes, you are not able to run Firefox from the root user account. On host H1, use the switch user command to switch from the root user to the analyst user account:

[root@secOps analyst]# **su analyst**

1. Start the web browser on H1. This will take a few moments.


[analyst@secOps ~]$ **firefox &**

****


1. After the Firefox window opens, start a tcpdump session in the terminal **Node: H1** and send the output to a file called **capture.pcap**. With the -v option, you can watch the progress. This capture will stop after capturing 50 packets, as it is configured with the option -c 50.

[analyst@secOps ~]$ **sudo tcpdump -i H1-eth0 -v -c 50 -w**

### /home/analyst/capture.pcap



1. After the tcpdump starts, quickly navigate to 172.16.0.40 in the Firefox web browser.




# Part 2: Analyze the Packets using Wireshark

## Step 1: Apply a filter to the saved capture.

1. Press ENTER to see the prompt. Start Wireshark on **Node: H1**. Click **OK** when prompted by the warning regarding running Wireshark as superuser.

[analyst@secOps ~]$ **wireshark &**


1. In Wireshark, click **File** > **Open**. Select the saved pcap file located at /home/analyst/capture.pcap.
2. Apply a **tcp** filter to the capture. In this example, the first 3 frames are the interested traffic.



## Step 2: Examine the information within packets including IP addresses, TCP port numbers, and TCP control flags.

1. In this example, frame 1 is the start of the three-way handshake between the PC and the server on H4. In the packet list pane (top section of the main window), select the first packet, if necessary.
2. Click the **arrow** to the left of the Transmission Control Protocol in the packet details pane to expand it and examine the TCP information. Locate the source and destination port information.
3. Click the **arrow** to the left of the Flags. A value of 1 means that flag is set. Locate the flag that is set in this packet.

**Note**: You may have to adjust the top and middle windows sizes within Wireshark to display the necessary information.



What is the TCP source port number?

33310

How would you classify the source port?

The source port is a 16-bit number used by the sending application or device to uniquely identify itself when establishing a connection or sending data packets.

What is the TCP destination port number?

80

How would you classify the destination port?

The destination port is also a 16-bit number that identifies the intended recipient application or service on the receiving end.


Which flag (or flags) is set?

0x002 (SYN)

What is the relative sequence number set to?

0

1. Select the next packet in the three-way handshake. In this example, this is frame 2. This is the web server replying to the initial request to start a session.



What are the values of the source and destination ports?


80 and 33310

Which flags are set?

0x012 (SYN, ACK)

What are the relative sequence and acknowledgment numbers set to?

0 and 1Finally, select the third packet in the three-way handshake.



Examine the third and final packet of the handshake

Which flag (or flags) is set?

0x010 (ACK)

The relative sequence and acknowledgment numbers are set to 1 as a starting point. The TCP connection is established and communication between the source computer and the web server can begin.

# Part 3: View the packets using tcpdump

You can also view the pcap file and filter for the desired information.

1. Open a new terminal window, enter **man tcpdump**. **Note**: You may need to press ENTER to see the prompt.

Using the manual pages available with the Linux operating system, you read or search through the manual pages for options for selecting the desired information from the pcap file.

[analyst@secOps ~]$ **man tcpdump**

TCPDUMP(1) General Commands Manual TCPDUMP(1)

NAME

tcpdump - dump traffic on a network

SYNOPSIS

tcpdump [ -AbdDefhHIJKlLnNOpqStuUvxX# ] [ -B buffer\_size ] [ -c count ]

[ -C file\_size ] [ -G rotate\_seconds ] [ -F file ]

[ -i interface ] [ -j tstamp\_type ] [ -m module ] [ -M secret ] [ --number ] [ -Q in|out|inout ]

[ -r file ] [ -V file ] [ -s snaplen ] [ -T type ] [ -w file ] [ -W filecount ]

[ -E spi@ipaddr algo:secret,... ]

[ -y datalinktype ] [ -z postrotate-command ] [ -Z user ] [ --time-stamp-precision=tstamp\_precision ]

[ --immediate-mode ] [ --version ] [ expression ]

<some output omitted>

To search through the man pages, you can use / (searching forward) or ? (searching backward) to find specific terms, and **n** to forward to the next match and **q** to quit. For example, search for the information on the switch -r, type **/-r**. Type **n** to move to the next match.

What does the switch **-r** do?

Read packets from file

1. In the same terminal, open the capture file using the following command to view the first 3 TCP packets captured:

[analyst@secOps ~]$ **tcpdump -r /home/analyst/capture.pcap tcp -c 3**

reading from file capture.pcap, link-type EN10MB (Ethernet)

13:58:30.647462 IP 10.0.0.11.58716 > 172.16.0.40.http: Flags [S], seq 2432755549, win

29200, options [mss 1460,sackOK,TS val 3864513189 ecr 0,nop,wscale 9], length 0

13:58:30.647543 IP 172.16.0.40.http > 10.0.0.11.58716: Flags [S.], seq 1766419191, ack

2432755550, win 28960, options [mss 1460,sackOK,TS val 50557410 ecr

3864513189,nop,wscale 9], length 0

13:58:30.647544 IP 10.0.0.11.58716 > 172.16.0.40.http: Flags [.], ack 1, win 58,

options [nop,nop,TS val 3864513189 ecr 50557410], length 0

To view the 3-way handshake, you may need to increase the number of lines after the **-c** option.

1. Navigate to the terminal used to start Mininet. Terminate the Mininet by entering quit in the main CyberOps VM terminal window.

mininet> **quit**

\*\*\* Stopping 0 controllers

\*\*\* Stopping 2 terms

\*\*\* Stopping 5 links

|  |  |  |
| --- | --- | --- |
| ..... |  | |
| \*\*\* Stopping | 1 | switches |
| s1 |  |  |
| \*\*\* Stopping | 5 | hosts |

H1 H2 H3 H4 R1

\*\*\* Done [analyst@secOps ~]$

1. After quitting Mininet, enter **sudo mn -c** to clean up the processes started by Mininet. Enter the password

**cyberops** when prompted.

[analyst@secOps ~]$ **sudo mn -c**

[sudo] password for analyst:

# Reflection Questions

1. There are hundreds of filters available in Wireshark. A large network could have numerous filters and many different types of traffic. List three filters that might be useful to a network administrator.

=Filter by specific protocols such as TCP, UDP, ICMP, or a particular application layer protocol like HTTP, DNS, or SMTP. This allows network administrators to focus on traffic relevant to a particular protocol, helping in troubleshooting or monitoring specific services. Exemple: tcp.port ==80

1. What other ways could Wireshark be used in a production network?

* Wireshark can be used to analyze network performance by capturing and analyzing traffic patterns, identifying latency issues, and monitoring bandwidth usage. This is crucial for ensuring optimal network performance.
* Wireshark can be employed as a security tool to detect and analyze malicious activities on the network. It can help in identifying suspicious traffic, detecting anomalies, and investigating potential security incidents.